Detailed Procedures

Storage tank cleaning procedure:

 The sediment shall be drained every *four months* by opening the gate valve located at the base of the storage tank. The water shall be discharged for at least *two full minutes* or until the water is clear and free of visible particles which ever is longer. If the flushing takes more than *fifteen minutes*, then the storage tank shall be drained and cleaned in accordance with AWWA Standard C652-92.

Replacement of any system components shall be done following all applicable Standards and Guidance documents.